#!/bin/sh
steps="5"
device="intel_backlight"
delay="125000"

case "$1" in
	increase) brillo -s $device -u $delay -q -A $steps ;;
	decrease) brillo -s $device -u $delay -q -U $steps ;;
	-h|*) echo "usage: setbr increase|decrease" >&2; exit 1; ;;
esac

pkill -RTMIN+4 slstatus
